# DIOT CompactPCI Serial crate hardware

DIOT 3U crate mechanics and backplane compliant with CompactPCI-Serial standard.

## 3D Viewer
For component 3D Model rendering, make sure your KISYS3DMOD variable points to the location of the CERN library with *.stp files.

### To-do
JP1 from the power_backplane does not come from the CERN libraries, please change it for consistency - all components from the same set of libraries.
