
.. _spec7_driver:

SPEC7 Driver(s)
==============

Driver(s) Structure
-------------------

.. _at24:

AT24 DRIVER
	Inbuilt module provided with kernel and can be loaded using modprobe
.. _code_block::

	`modprobe at24`


.. _i2c_ocore:

I2C OCORE
  This is the driver for the I2C OCORE IP-core. It is used to communicate with
  the standard FMC EEPROM available what on FMC modules. The driver is
  available in Linux but also (as a backport) in `general cores`_.

.. _spec7_core:

SPEC7_CORE
  This is initial core driver for SPEC7 to enumerate PCIe and initialise I2C EEPROM

.. _xdma:
XDMA
  DMA IP Core driver provided by Xilinx `dma ip drivers`_ 
  

.. _`general cores`:https://ohwr.org/project/general-cores
.. _`dma ip drivers`:https://github.com/Xilinx/dma_ip_drivers/tree/2019.2



